***ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

Contract title: Supply of biomedical equipments

 **p 1 /…**

**Publication reference:** 14/CUAMM/ETH/2025/AID 05/12282/ETH

**Columns 1-2 should be completed by the contracting authority Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

Lot 1 Supply of Bio medical equipment

| **1.****Item number** | **2.****Specifications required** | **3.****Specifications offered** | **4.****Notes, remarks, ref to documentation** | **5.****Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| 1 | Fuses set European 5x20Specification- type T Different ratings for various devices da 1A a 20AQuantity = 60 |  |  |  |
| 2 | Fuses set American 6.3x32Specification- Different ratings for various devices da 1A a 20AQuantity = 30 |  |  |  |
| 3 | Fuses UKSpecification-13A Quantity = 25 |  |  |  |
| 4 |  Batteries Specification- Standard battery types (AA, AAA, 9V)Quantity = 30 |  |  |  |
| 5 | Plastic O-ringsSpecification- set used in mechanical sealsQuantity = 20 |  |  |  |
| 6 | Final Bacterial filterSpecification- Different size (for Suction, O2 concentration, ventilator)Quantity = 50 |   |  |  |
| 7 | TubingSpecification : Plastic Connector Tube different size (for Suction, O2 concentration, ventilator)Quantity = 70 |  |  |  |
| 8 | Power cablesSpecifications:Type F 15A fuse 13A IEC 60320 C13Quantity = 14 |  |  |  |
| 9 | Power stripSpecifications: Type F (for OR)Quantity = 10 |  |  |  |
| 10 | halogen lightSpecifcation: 6v 20w halogen lamp , ID:olympus cx23 (for microscope)Quantity =10 |  |  |  |
| 11 | Autoclave heaterSpecifcation:2000 Watt photo. ID:medicraft (for autoclave)Quantity = 13 |  |  |  |
| 12 | LightSpecifcation: 24v 100w halogen (for OR lamp)Quantity = 10 |  |  |  |
| 13 | pulse oximeter sensorSpecifcation: sensor, ID: red5 masimo (for Pediatrics, NICU and Emergency)Quantity = 10 |  |  |  |
| 14 | ContainerSpecifcation: Suction 7A-23D yuwell (for suction machine)Quantity = 4 |  |  |  |
| 15 | ESU penSpecifcation: OR cut pen 3 pin, ID: beilin dgd-300b-2Quantity = 2 |  |  |  |
| 16 | Display LCDSpecifcation: with HDMI + extender , ID: sonoacex7 (for ultrasound)Quantity = 1 |  |  |  |
| 17 | Temperature sensorSpecifcation: BN-100 jack connector, ID: BN-100 (For Infant warmer)Quantity = 3 |  |  |  |
| 18 | Temperature sensor jackSpecifcation: female connector, ID: BN-100 (for Infant warmer)Quantity = 1 |  |  |  |
| 19 | Temperature sensorSpecifcation: 3 pin connector, ID: phoenix (for Infant warmer)Quantity = 1 |  |  |  |
| 20 | Power cablesSpecifcation: Type G 15A fuse 13A IEC 60320 C13 (for Infant warmer)Quantity = 5 |  |  |  |
| 21 | Autoclave heaterSpecifcation: <2000 watt photo, ID: heuer (for autoclave) Quantity = 4 |  |  |  |
| 22 | Autoclave heaterSpecifcation: 3 heater < 4000Watt photo, ID: ls-b75l-I (for autoclave)Quantity = 1 |  |  |  |
| 23 | LensSpecifcation: 10x 20x 40x 100x Clarify lens type objective lens, ID: primo start (for microscope)Quantity = 1 |  |  |  |
| 24 | RelaySpecifcation: 220v 15/20A, ID: sturday (for autoclave)Quantity = 2 |  |  |  |
| 25 | Radient WarmerIR lamp/Heater lamp for radiant warmerSpecifcation: IR lamp/Heater lamp 600W con reflactor:, ID: phoenix (for infant warmer)Quantity = 4 |  |  |  |
| 26 | PM sensorsSpecifcation: accessories( ECG leads, SpO2, BP), ID:anyview a8 (for patient monitor)Quantity = 3 |  |  |  |