***ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

Contract title: Supply of biomedical equipments

**p 1 /…**

**Publication reference:** 14/CUAMM/ETH/2025/AID 05/12282/ETH

**Columns 1-2 should be completed by the contracting authority Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

Lot 1 Supply of Bio medical equipment

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| 1 | Fuses set European 5x20  Specification- type T Different ratings for various devices da 1A a 20A  Quantity = 60 |  |  |  |
| 2 | Fuses set American 6.3x32  Specification- Different ratings for various devices da 1A a 20A  Quantity = 30 |  |  |  |
| 3 | Fuses UK  Specification-13A  Quantity = 25 |  |  |  |
| 4 | Batteries  Specification- Standard battery types (AA, AAA, 9V)  Quantity = 30 |  |  |  |
| 5 | Plastic O-rings  Specification- set used in mechanical seals  Quantity = 20 |  |  |  |
| 6 | Final Bacterial filter  Specification- Different size (for Suction, O2 concentration, ventilator)  Quantity = 50 |  |  |  |
| 7 | Tubing  Specification : Plastic Connector Tube different size (for Suction, O2 concentration, ventilator)  Quantity = 70 |  |  |  |
| 8 | Power cables  Specifications:  Type F 15A fuse 13A IEC 60320 C13  Quantity = 14 |  |  |  |
| 9 | Power strip  Specifications: Type F (for OR)  Quantity = 10 |  |  |  |
| 10 | halogen light  Specifcation: 6v 20w halogen lamp , ID:olympus cx23 (for microscope)  Quantity =10 |  |  |  |
| 11 | Autoclave heater  Specifcation:2000 Watt photo. ID:medicraft (for autoclave)  Quantity = 13 |  |  |  |
| 12 | Light  Specifcation: 24v 100w halogen (for OR lamp)  Quantity = 10 |  |  |  |
| 13 | pulse oximeter sensor  Specifcation: sensor, ID: red5 masimo (for Pediatrics, NICU and Emergency)  Quantity = 10 |  |  |  |
| 14 | Container  Specifcation: Suction 7A-23D yuwell (for suction machine)  Quantity = 4 |  |  |  |
| 15 | ESU pen  Specifcation: OR cut pen 3 pin, ID: beilin dgd-300b-2  Quantity = 2 |  |  |  |
| 16 | Display LCD  Specifcation: with HDMI + extender , ID: sonoacex7 (for ultrasound)  Quantity = 1 |  |  |  |
| 17 | Temperature sensor  Specifcation: BN-100 jack connector, ID: BN-100 (For Infant warmer)  Quantity = 3 |  |  |  |
| 18 | Temperature sensor jack  Specifcation: female connector, ID: BN-100 (for Infant warmer)  Quantity = 1 |  |  |  |
| 19 | Temperature sensor  Specifcation: 3 pin connector, ID: phoenix (for Infant warmer)  Quantity = 1 |  |  |  |
| 20 | Power cables  Specifcation: Type G 15A fuse 13A IEC 60320 C13 (for Infant warmer)  Quantity = 5 |  |  |  |
| 21 | Autoclave heater  Specifcation: <2000 watt photo, ID: heuer (for autoclave)  Quantity = 4 |  |  |  |
| 22 | Autoclave heater  Specifcation: 3 heater < 4000Watt photo, ID: ls-b75l-I (for autoclave)  Quantity = 1 |  |  |  |
| 23 | Lens  Specifcation: 10x 20x 40x 100x Clarify lens type objective lens, ID: primo start (for microscope)  Quantity = 1 |  |  |  |
| 24 | Relay  Specifcation: 220v 15/20A, ID: sturday (for autoclave)  Quantity = 2 |  |  |  |
| 25 | Radient Warmer  IR lamp/Heater lamp for radiant warmer  Specifcation: IR lamp/Heater lamp 600W con reflactor:, ID: phoenix (for infant warmer)  Quantity = 4 |  |  |  |
| 26 | PM sensors  Specifcation: accessories( ECG leads, SpO2, BP), ID:anyview a8 (for patient monitor)  Quantity = 3 |  |  |  |