# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Heavy Duty Generator p 1 /…**

**Publication reference: 010/CUAMM/ETH/2023**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

Lot 1 Heavy Duty Generator

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| 1 | Heavy Duty Generator Set, Technical Specifications,   * PrimePower 250 KVA/200 KW * Standby power 275 KVA/220 KW * 3Phase, * Silent, 1500 rpm   Financial Offer   * Minimum one-year warranty * Service maintenance * Availability of spare parte * Transport, Installation, testing and commissioning   Quantity:1  Delivery and Installation: Wollisso St. Luke Catholic Hospital |  |  |  |