***ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

**Contract title: Supply of Medical Equipment and Consumable**

**p 1 /…**

**Publication reference:** 43/CUAMM/ETH/2024

**Columns 1-2 should be completed by the contracting authority Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

**Lot 1 Medical Equipment**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item number** | | **2.**  **Specifications required** | **3.**  **Specifications offered**  **TO BE FILLED BY THE SUPPLIER** | **4.**  **Notes, remarks, ref. to documentation** | **5.**  **Evaluation committee’s notes** |
|  | **Glucometer with test strips**  **Specification:**  Zero setting between measurements  Sample size of 5-10 uL (capillary, venous or arterial whole blood)  Reading time**:** 10sec-5min supplied with lancets and test strips specified below  **Quantity: 1**  Delivery place: Addis Ababa | | Delivery time: (TO BE FILLED) |  |  |
|  | **Measuring tape (tape measure/medical)**  **Specification**:  Length 2,000 mm (1 mm spacing) /60 inches  Push button retraction, features both inches and centimetres  **Quantity: 1**  Delivery place: Addis Ababa | | Delivery time: (TO BE FILLED) |  |  |
|  | **Monofilament\_Medical**  **Specification:** 5.07 gm nylon monofilament ( to test sensation over foot)  **Quantity: 1**  Delivery place: Addis Ababa | | Delivery time: (TO BE FILLED) |  |  |
| **4.** | **Adult BP Apparatus**  **Specification**:Digital  Complete with adult cuff, bulb and value in vinyl case ( typical dimensions (0.15x0.15x0.04 cm)  Weight 0.30 kg  **Quantity: 1**  Delivery place: Addis Ababa | | Delivery time: (TO BE FILLED) |  |  |
| **5.** | **Stethoscope**  **Specification**:  Stethoscope has stainless steel/ chromed brass  Double-bell chest piece (dual-use adult and paediatric auscultation).  Adult diaphragm: approx 43 mm.  Pediatric diaphragm: approx 28 mm.  Sensitivity, 50 to 500 Hz: 3.2 dB (cardiology). Sensitivity, 600 to 1500 Hz: 8.1 dB (pneumology).  Single tube in treated rubber, lumen diameter: approx 10 mm.  Y-part is reinforced with stainless steel spring attached to the rigid ear tubes.  Spring is treated to give long lasting rebound and comfort.  Ear tubes are made of stainless steel or chromed brass.  Ear-pieces are made of plastic and are removable.  Total length, approx 70 cm.  **Quantity: 1**  Delivery place: Addis Ababa | | Delivery time: (TO BE FILLED) |  |  |

**Lot 2: Medical Consumables**

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
|  | Test strips:  **Specification:** One packet of 50 strips  Brand has to match glucometer  **Quantity: 1**  Delivery place: Addis Ababa | Delivery time: (TO BE FILLED) |  |  |
|  | Blood lancet: Safe, disposable/single use, sterile 50 pcs in one  Length approx. 40 mm Width approx: 6mm  **Quantity: 1**  Delivery place: Addis Ababa | Delivery time: (TO BE FILLED) |  |  |